;========================================== 
; This is a Setup information file for monitors  with ICM  file; 
; Copyright (c) 2022 ASROCK  Corporation

;==========================================
 
[version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%ASROCK%
CatalogFile=PG34WQ15R2B.cat   
DriverVer=03/24/2022,1.0.0.0

[ControlFlags]

ExcludeFromSelect.nt=Monitor\ASRAAA2
ExcludeFromSelect.nt=Monitor\ASRAAA2

[DestinationDirs]
DefaultDestDir=11
PG34WQ15R2B_HDMI.CopyFiles=23
PG34WQ15R2B_DP.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,

[SourceDisksFiles]
PG34WQ15R2B.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%ASROCK%=ASROCK,NTx86, NTamd64

[ASROCK]
%PG34WQ15R2B_HDMI%=PG34WQ15R2B_HDMI.Install, Monitor\ASRAAA2
%PG34WQ15R2B_DP%=PG34WQ15R2B_DP.Install, Monitor\ASRAAA2

[ASROCK.NTx86]
%PG34WQ15R2B_HDMI%=PG34WQ15R2B_HDMI.Install, Monitor\ASRAAA2
%PG34WQ15R2B_DP%=PG34WQ15R2B_DP.Install, Monitor\ASRAAA2


[ASROCK.NTamd64]
%PG34WQ15R2B_HDMI%=PG34WQ15R2B_HDMI.Install, Monitor\ASRAAA2
%PG34WQ15R2B_DP%=PG34WQ15R2B_DP.Install, Monitor\ASRAAA2

[PG34WQ15R2B_HDMI.Install]
DelReg=DEL_CURRENT_REG
AddReg=PG34WQ15R2B_HDMI.AddReg
Copyfiles=PG34WQ15R2B_HDMI.CopyFiles

[PG34WQ15R2B_DP.Install]
DelReg=DEL_CURRENT_REG
AddReg=PG34WQ15R2B_DP.AddReg
Copyfiles=PG34WQ15R2B_DP.CopyFiles


[PG34WQ15R2B_HDMI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[PG34WQ15R2B_DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install



[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[PG34WQ15R2B_HDMI.AddReg]
HKR,"MODES\3440,1440",Mode1,,"30.0-160.0,48.0-100.0,+,+"
HKR,,MaxResolution,,"3440,1440"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"PG34WQ15R2B.icm"
HKR,,DisplayHdrLevel, %REG_MULTI_SZ_APPEND%, AE040E1F-51EC-4CAC-8501-E611C3C29CFE

[PG34WQ15R2B_DP.AddReg]
HKR,"MODES\3440,1440",Mode1,,"260.0-260.0,48.0-165.0,+,+"
HKR,,MaxResolution,,"3440,1440"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"PG34WQ15R2B.icm"
HKR,,DisplayHdrLevel, %REG_MULTI_SZ_APPEND%, AE040E1F-51EC-4CAC-8501-E611C3C29CFE



[PG34WQ15R2B_HDMI.CopyFiles]
PG34WQ15R2B.icm

[PG34WQ15R2B_DP.CopyFiles]
PG34WQ15R2B.icm



[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

ASROCK="ASROCK"
Diskname="ASROCK PG34WQ15R2B Monitor installation diskette"
REG_MULTI_SZ_APPEND=0x00010008

PG34WQ15R2B_HDMI="PG34WQ15R2B"
PG34WQ15R2B_DP="PG34WQ15R2B"