;=======================================================
; X22-1 CAM.INF Ver. 1.0 10/31/2017
;
; Monitor INF file for Fujitsu Display X22-1 CAM
;
; Copyright 2017 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FUS-Mfg%
CatalogFile = X22-1 CAM.cat
DriverVer   = 10/31/2017, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
X22-1 CAM.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
X22-1 CAM.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS08BA
ExcludeFromSelect = Monitor\FUS08BB

[Manufacturer]
%FUS-Mfg% = FUS-Mfg, NTx86, NTAMD64

[FUS-Mfg]

%X22-1 CAM.VGA%  = X22-1 CAM.VGA.Install, Monitor\FUS08BA
%X22-1 CAM.DP%     = X22-1 CAM.DP.Install, Monitor\FUS08BB

[FUS-Mfg.NTx86]
%X22-1 CAM.VGA%  = X22-1 CAM.VGA.Install, Monitor\FUS08BA
%X22-1 CAM.DP%     = X22-1 CAM.DP.Install, Monitor\FUS08BB

[FUS-Mfg.NTAMD64]
%X22-1 CAM.VGA%  = X22-1 CAM.VGA.Install, Monitor\FUS08BA
%X22-1 CAM.DP%     = X22-1 CAM.DP.Install, Monitor\FUS08BB

[X22-1 CAM.VGA.Install]
DelReg    = FUS_CURRENT_REG
AddReg    = X22-1 CAM.VGA.AddReg, 1920x1080, DPMS
CopyFiles = X22-1 CAM.CopyFiles

[X22-1 CAM.DP.Install]
DelReg    = FUS_CURRENT_REG
AddReg    = X22-1 CAM.DP.AddReg, 1920x1080, DPMS
CopyFiles = X22-1 CAM.CopyFiles

[FUS_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[X22-1 CAM.VGA.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"X22-1 CAM.icm"

[X22-1 CAM.DP.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"X22-1 CAM.icm"

[1920x1080]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[X22-1 CAM.CopyFiles]
X22-1 CAM.icm

[X22-1 CAM.VGA.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[X22-1 CAM.DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FUS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

X22-1 CAM.VGA= "Fujitsu X22-1 CAM (VGA)"
X22-1 CAM.DP = "Fujitsu X22-1 CAM (DP)"
