; ---------------------------------------------------------------------
; scb7000.inf - INF file for PCIe DVR board driver.
;
;
; ---------------------------------------------------------------------


[Version]
Signature     = "$WINDOWS NT$"
Class         = Media
ClassGuid     = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider      = DVR
DriverVer     = 07/29/2011, 7.0.1.3
CatalogFile.NTAMD64  = scb7000.cat


[Manufacturer]
%DVR%     = DVR , NTx86, NTamd64


[DVR.NTx86]
%DVR16.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_00007016
%DVR8.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_00007008
%DVR4.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0004&SUBSYS_00007004
%DVR7116.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_00007116
%DVR7108.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_00007108
%DVR16S.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007016
%DVR8S.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007008
%DVR4S.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007004
%DVR4SHD.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0024&SUBSYS_00008004
%PCI\VEN_18A2&DEV_0002&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0003&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0004&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0004&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0010&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0010&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0006&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0006&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0011&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0011&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0020&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0024&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0024&SUBSYS_000018A2


[DVR.NTamd64]
%DVR16.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_00007016
%DVR8.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_00007008
%DVR4.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0004&SUBSYS_00007004
%DVR7116.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_00007116
%DVR7108.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_00007108
%DVR16S.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007016
%DVR8S.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007008
%DVR4S.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_00007004
%DVR4SHD.Desc%  = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0024&SUBSYS_00008004
%PCI\VEN_18A2&DEV_0002&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0002&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0003&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0003&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0004&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0004&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0010&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0010&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0006&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0006&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0011&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0011&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0020&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0020&SUBSYS_000018A2
%PCI\VEN_18A2&DEV_0024&SUBSYS_000018A2.Desc% = PCIE_DVR.Install, PCI\VEN_18A2&DEV_0024&SUBSYS_000018A2


;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 2000

[PCIE_DVR.Install]
CopyFiles    = PCIE_DVR.Files.Driver

[PCIE_DVR.Files.Driver]
scb7000.sys


[PCIE_DVR.Install.Services]
AddService   = PCIE_DVR, %SPSVCINST_ASSOCSERVICE%, PCIE_DVR.Service

[DestinationDirs]
PCIE_DVR.Files.Driver    = 10,System32\Drivers

[SourceDisksNames]
1 = %SourceDiskName%,,,

[SourceDisksFiles]
scb7000.sys = 1

[PCIE_DVR.Service]
DisplayName     = %PCIE_DVR.ServiceName%
ServiceType     = %SERVICE_KERNEL_DRIVER%
StartType       = %SERVICE_DEMAND_START%
ErrorControl    = %SERVICE_ERROR_NORMAL%
ServiceBinary   = %10%\System32\Drivers\scb7000.sys


;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Strings

[Strings]
PCIE_DVR                = "PCIe DVR Board Driver"
PCIE_DVR.ServiceName    = "PCIe DVR Board Driver"

SPSVCINST_ASSOCSERVICE       = 0x00000002
COPYFLG_NOSKIP               = 2     ; Do not allow user to skip file
SERVICE_KERNEL_DRIVER        = 1
SERVICE_AUTO_START           = 2
SERVICE_DEMAND_START         = 3
SERVICE_ERROR_NORMAL         = 1

DVR16.Desc   = "PCIe 16CH DVR Board"
DVR8.Desc    = "PCIe 8CH DVR Board"
DVR4.Desc    = "PCIe 4CH DVR Board"
DVR7116.Desc = "PCIe 16CH DVR TVout Board"
DVR7108.Desc = "PCIe 8CH DVR TVout Board"
;DVR.Desc     = "PCIe DVR Board"
DVR16S.Desc   = "PCIe 16CH DVR Board V2"
DVR8S.Desc    = "PCIe 8CH DVR Board V2"
DVR4S.Desc    = "PCIe 4CH DVR Board V2"
DVR4SHD.Desc  = "PCIe 4CH HD DVR Board V2"


DVR			= "DVR"
SourceDiskName = "DVR Install Directory"

PCI\VEN_18A2&DEV_0002&SUBSYS_000018A2.Desc   = "Stretch VRC6016 DVR Card"
PCI\VEN_18A2&DEV_0003&SUBSYS_000018A2.Desc   = "Stretch VRC6008 DVR Card"
PCI\VEN_18A2&DEV_0004&SUBSYS_000018A2.Desc   = "Stretch VRC6004 DVR Card"
PCI\VEN_18A2&DEV_0010&SUBSYS_000018A2.Desc   = "Stretch VRC6404HD DVR Card"
PCI\VEN_18A2&DEV_0006&SUBSYS_000018A2.Desc   = "Stretch VRC6416 DVR Card"
PCI\VEN_18A2&DEV_0011&SUBSYS_000018A2.Desc   = "Stretch VRC6004HD DVR Card"
PCI\VEN_18A2&DEV_0020&SUBSYS_000018A2.Desc   = "Stretch VRC7016L DVR Card"
PCI\VEN_18A2&DEV_0024&SUBSYS_000018A2.Desc   = "PCIe 4CH HD DVR Board V2"

