; Atmel INF File for USB HID devices
;
; Add selective suspend feature to Atmel HID
;

[Version]
Signature            = "$Windows NT$"
Provider             = %ATML%
Class                = HIDClass
CLASSGUID            = {745a17a0-74d3-11d0-b6fe-00a0c90f57da};
DriverVer            = 08/13/2014,1.8.0.1
CatalogFile.NT       = AtmelHID.CAT

[Manufacturer]
%ATML% = Atmel,NTx86.6.1,NTamd64.6.1,NTx86.6.2,NTamd64.6.2,NTx86.6.3,NTamd64.6.3

[Atmel.NTx86.6.3]
; Windows 8.1 not supported

[Atmel.NTamd64.6.3]
; Windows 8.1 not supported

[Atmel.NTx86.6.2]
; Windows 8.0 not supported

[Atmel.NTamd64.6.2]
; Windows 8.0 not supported

[Atmel.NTx86.6.1]

; Windows 7.0 32bit

;mXT2952T, PID 0x2148
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&MI_00

;mXT1664S, PID 0x212C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&MI_00

;mXT1664T, PID 0x2149
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&MI_00

;mXT2952T2, PID 0x214E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&MI_00

;mXT1664S, PID 0x840B
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&MI_00

;mXT2952T, PID 0x8820
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&MI_00

;mXT2952T, PID 0x8821
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&MI_00

;mXT3432S, PID 0x881F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&MI_00

;mXT2952T, PID 0x8A06
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&MI_00

;mXT2952T, PID 0x8A07
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&MI_00

;mxt1664S mxt1188S, PID 0x844F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&MI_00

;mxt2952T, PID 0x8A2C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&MI_00

;mxt2952T, PID 0x8A2D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&MI_00

;mxt2952T, PID 0x8A2E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&MI_00

;mxt2952T, PID 0x8A2F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&MI_00

;mxt2952T, PID 0x8A30
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&MI_00

;mxt2952T, PID 0x8A33
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&MI_00

;mxt2952T, PID 0x8A37
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&MI_00

;mxt2952T, PID 0x8A39
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&MI_00

;mxt2952T, PID 0x8A3A
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&MI_00

;mxt2952T, PID 0x8A3B
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&MI_00

;mxt2952T, PID 0x8A3C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&MI_00

;mxt2952T, PID 0x8A3D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&MI_00

;mxt2952T, PID 0x8A3E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&MI_00

;mxt2952T, PID 0x8A3F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&MI_00

;mxt2952T, PID 0x8A40
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&MI_00

;mxt1664T, PID 0x8A44
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&MI_00

;mxt1664T, PID 0x8A45
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&MI_00

;mxt2952T, PID 0x8A46
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&MI_00

;mxt2952T, PID 0x8A47
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&MI_00

;mxt2952T, PID 0x8A48
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&MI_00

;mxt2952T, PID 0x8A49
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&MI_00

;mxt2952T, PID 0x8A4A
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&MI_00

;mxt2952T, PID 0x8A4D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&MI_00

;mxt2952T2, PID 0x8A80
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&MI_00

;mxt2952T2, PID 0x8A81
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&MI_00

;mxt2952T2, PID 0x8A82
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&MI_00

;mxt2952T2, PID 0x8A84
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&MI_00


[Atmel.NTamd64.6.1]
; Windows 7.0 64bit

;mXT2952T, PID 0x2148
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2148&MI_00

;mXT1664S, PID 0x212C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_212C&MI_00

;mXT1664T, PID 0x2149
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_2149&MI_00

;mXT2952T2, PID 0x214E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_214E&MI_00

;mXT1664S, PID 0x840B
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_840B&MI_00

;mXT2952T, PID 0x8820
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8820&MI_00

;mXT2952T, PID 0x8821
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8821&MI_00

;mXT3432S, PID 0x881F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_881F&MI_00

;mXT2952T, PID 0x8A06
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A06&MI_00

;mXT2952T, PID 0x8A07
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A07&MI_00

;mxt1664S mxt1188S, PID 0x844F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_844F&MI_00

;mxt2952T, PID 0x8A2C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2C&MI_00

;mxt2952T, PID 0x8A2D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2D&MI_00

;mxt2952T, PID 0x8A2E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2E&MI_00

;mxt2952T, PID 0x8A2F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A2F&MI_00

;mxt2952T, PID 0x8A30
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A30&MI_00

;mxt2952T, PID 0x8A33
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A33&MI_00

;mxt2952T, PID 0x8A37
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A37&MI_00

;mxt2952T, PID 0x8A39
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A39&MI_00

;mxt2952T, PID 0x8A3A
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3A&MI_00

;mxt2952T, PID 0x8A3B
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3B&MI_00

;mxt2952T, PID 0x8A3C
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3C&MI_00

;mxt2952T, PID 0x8A3D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3D&MI_00

;mxt2952T, PID 0x8A3E
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3E&MI_00

;mxt2952T, PID 0x8A3F
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A3F&MI_00

;mxt2952T, PID 0x8A40
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A40&MI_00

;mxt1664T, PID 0x8A44
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A44&MI_00

;mxt1664T, PID 0x8A45
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A45&MI_00

;mxt2952T, PID 0x8A46
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A46&MI_00

;mxt2952T, PID 0x8A47
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A47&MI_00

;mxt2952T, PID 0x8A48
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A48&MI_00

;mxt2952T, PID 0x8A49
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A49&MI_00

;mxt2952T, PID 0x8A4A
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4A&MI_00

;mxt2952T, PID 0x8A4D
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A4D&MI_00

;mxt2952T2, PID 0x8A80
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A80&MI_00

;mxt2952T2, PID 0x8A81
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A81&MI_00

;mxt2952T2, PID 0x8A82
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A82&MI_00

;mxt2952T2, PID 0x8A84
%AtmelHIDClient_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&REV_*&MI_01
%AtmelHIDFW_1%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&MI_01
%AtmelHIDClient_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&REV_*&MI_00
%AtmelHIDFW_2%=HID_SelSus_Inst, USB\VID_03EB&PID_8A84&MI_00


; Windows Service Installation Section

[HID_SelSus_Inst.NT]
Include =	input.inf
Needs = 	HID_Inst.NT


[HID_SelSus_Inst.NT.HW]
AddReg = HID_SelSus_Inst.AddReg.NT.HW

[HID_SelSus_Inst.AddReg.NT.HW]
HKR,,"SelectiveSuspendEnabled",0x00000001,0x1
HKR,,"SystemWakeEnabled",0x00010001,1
HKR,,"AllowIdleIrpInD3",0x00000001,0x1

[HID_SelSus_Inst.NT.Services]
Include = 	input.inf
Needs = HID_SelSus_Inst.NT.Services

;[HID_SelSus_Inst.NT.Services]
;AddService = HidUsb,%SPSVCINST_ASSOCSERVICE%,HID_Service_Inst

;[HID_Inst.NT]
;Copyfiles = HID_Inst.CopyFiles.NT

;[HID_Inst.NT.HW]
;DelReg = HID_Inst.DelReg.NT.HW

;[HID_Inst.CopyFiles.NT]
;hidusb.sys,,,0x100
;hidclass.sys,,,0x100
;hidparse.sys,,,0x100

;[HID_Inst.NT.Services]
;AddService = HidUsb,%SPSVCINST_ASSOCSERVICE%,HID_Service_Inst


[Strings]
ATML     = "Atmel"
AtmelHIDClient_1 = "Atmel Touchscreen Control"
AtmelHIDFW_1 = "Atmel Touchscreen Control"
AtmelHIDClient_2 = "Atmel Touchscreen Digitizer"
AtmelHIDFW_2 = "Atmel Touchscreen Digitizer"
;SPSVCINST_ASSOCSERVICE= 0x00000002