; Installation inf for the SEC SOC S3C2443X USB 2.0 Bulk IO Test B/D

[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%ProviderName%
DriverVer=07/028/2012

[SourceDisksNames]
1="USB Downloader Installation Disk for SEC SOC",,,

[SourceDisksFiles]
SADRV.sys = 1
SADRV.inf = 1

[Manufacturer]
%MfgName%=SystemLsi,NTamd64

[SystemLsi.NTamd64]
%USB\VID_5345&PID_1234.DeviceDesc%=SADRV.Dev, USB\VID_5345&PID_1234

;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
SADRV.Files.Ext = 10,System32\Drivers
SADRV.Files.Inf = 10,INF

[SADRV.Dev]
CopyFiles=SADRV.Files.Ext, SADRV.Files.Inf
AddReg=SADRV.AddReg

[SADRV.Dev.NT]
CopyFiles=SADRV.Files.Ext, SADRV.Files.Inf
AddReg=SADRV.AddReg

[SADRV.Dev.NT.Services]
Addservice = SADRV, 0x00000002, SADRV.AddService

[SADRV.AddService]
DisplayName    = %SADRV.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\SADRV.sys
LoadOrderGroup = Base

[SADRV.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SADRV.sys
HKLM,"System\Currentcontrolset\Services\SADRV\Parameters","MaximumTransferSize",0x10001,4096
HKLM,"System\Currentcontrolset\Services\SADRV\Parameters","DebugLevel",0x10001,2


[SADRV.Files.Ext]
SADRV.sys

[SADRV.Files.Inf]
SADRV.Inf


;---------------------------------------------------------------;

[Strings]
ProviderName="SEC AP application Team"
MfgName="SEC, SYSTEM LSI"
USB\VID_5345&PID_1234.DeviceDesc="Samkoon HMI Tech Corp."
SADRV.SvcDesc="SADRV.sys, SEC SOC USBD Driver"

