[Version]
Signature   = "$Windows NT$"
Class       = AndroidUsbDeviceClass
ClassGUID   = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider    = %ProviderName%
CatalogFile = qcadb.cat
DriverVer   = 09/19/2025,1.0.1.6
PnpLockdown = 1

[Manufacturer]
%ProviderName% = Standard, NTx86, NTamd64

[Standard.NTx86]
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0970&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0971&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0972&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0973&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0974&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0980&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0981&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0982&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0983&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0984&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0990&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0991&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0992&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0993&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0994&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1040&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1041&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1042&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1043&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1045&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1050&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1051&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1052&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1053&MI_01
%CompositeAdbInterface_cust_1054% = USB_Install, USB\VID_1BC7&PID_1054&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1055&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1056&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1057&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1058&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1060&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1061&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1062&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1063&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1067&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1070&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1071&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1072&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1073&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1074&MI_07
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1075&MI_00
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1076&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1077&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1078&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1079&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1080&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1081&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1082&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1083&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1084&MI_07
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1085&MI_00
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1086&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1095&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10A5&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10A9&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10AA&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10AB&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B0&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B1&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B2&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B3&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B5&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10C8&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10C9&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CA&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CB&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CD&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D0&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D1&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D2&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D3&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1200&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1201&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1203&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1204&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1206&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1208&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1212&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1216&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1217&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1221&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1222&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1223&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1230&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1231&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1232&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1234&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1235&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1260&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1261&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1262&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1980&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1981&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_3001&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_6000&MI_06
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_600A&MI_04
; Cinterion
%CompositeAdbInterface% = USB_Install, USB\VID_1E2D&PID_0104&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1E2D&PID_0105&MI_04
; Google
%SingleRecoveryInterface% = USB_Install, USB\VID_18D1&PID_D001
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D

[Standard.NTamd64]
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0970&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0971&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0972&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0973&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0974&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0980&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0981&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0982&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0983&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0984&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0990&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0991&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0992&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0993&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_0994&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1040&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1041&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1042&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1043&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1045&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1050&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1051&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1052&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1053&MI_01
%CompositeAdbInterface_cust_1054% = USB_Install, USB\VID_1BC7&PID_1054&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1055&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1056&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1057&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1058&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1060&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1061&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1062&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1063&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1067&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1070&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1071&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1072&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1073&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1074&MI_07
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1075&MI_00
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1076&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1077&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1078&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1079&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1080&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1081&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1082&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1083&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1084&MI_07
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1085&MI_00
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1086&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1095&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10A5&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10A9&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10AA&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10AB&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B0&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B1&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B2&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B3&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10B5&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10C8&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10C9&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CA&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CB&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10CD&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D0&MI_08
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D1&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D2&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_10D3&MI_09
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1200&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1201&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1203&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1204&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1206&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1208&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1212&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1216&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1217&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1221&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1222&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1223&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1230&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1231&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1232&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1234&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1235&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1260&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1261&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1262&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1980&MI_02
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1981&MI_05
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_3001&MI_04
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_6000&MI_06
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_600A&MI_04
; Cinterion
%CompositeAdbInterface% = USB_Install, USB\VID_1E2D&PID_0104&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1E2D&PID_0105&MI_04
; Google
%SingleRecoveryInterface% = USB_Install, USB\VID_18D1&PID_D001
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D

[ClassInstall32]
AddReg = ClassInstall_AddReg

[ClassInstall_AddReg]
HKR,,,,%ClassName%
HKR,,NoInstallClass,,1
HKR,,IconPath,0x00010000,"%%systemroot%%\system32\setupapi.dll,-20"
HKR,,LowerLogoVersion,,5.2

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include = winusb.inf
Needs   = WINUSB.NT.Services

[USB_Install.HW]
AddReg=Dev_AddReg,PwrMgmt_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[PwrMgmt_AddReg]
HKR,,DeviceIdleEnabled,0x00010001,1
HKR,,DefaultIdleState,0x00010001,1
HKR,,SystemWakeEnabled,0x00010001,1

[Strings]
ProviderName                = "Telit"
ClassName                   = "Android Device"
SingleAdbInterface          = "Android ADB Interface - Telit"
SingleRecoveryInterface     = "Android ADB Recovery Interface"
CompositeAdbInterface       = "Android Composite ADB Interface - Telit"
CompositeAdbInterface_cust_1054 = "SKT T-Login ADB Interface(FT980-KS)"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"

