; Remote NDIS template device setup file
; Copyright (c) Microsoft Corporation
;
; This is the template for the INF installation script  for the RNDIS-over-USB
; host driver that leverages the newer NDIS 6.x miniport (rndismp6.sys) for
; improved performance.
; and later operating systems on x86, amd64 and ia64 platforms.

[Version]
Signature           = "$Windows NT$"
Class               = Net
ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider            = %Microsoft%
DriverVer           = 11/26/2021,1.0.1.1
CatalogFile         = telit_rndis.cat
PnpLockdown         = 1

[Manufacturer]
%Microsoft%         = RndisDevices,NTx86,NTamd64,NTia64

; Decoration for x86 architecture
[RndisDevices.NTx86]
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0970&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0980&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0990&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1042&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1045&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1052&MI_00
%RndisDevice_cust_1054%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1054&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1056&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1062&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1072&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1079&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1082&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A6&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10AB&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10B2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C5&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10CB&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10D2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1203&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1231&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1251&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_2300&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1980&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1982

; Decoration for x64 architecture
[RndisDevices.NTamd64]
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0970&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0980&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_0990&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1042&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1045&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1052&MI_00
%RndisDevice_cust_1054%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1054&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1056&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1062&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1072&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1079&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1082&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A6&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10AB&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10B2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C5&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10CB&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10D2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1203&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1231&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1251&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_2300&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1980&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1982

; Decoration for ia64 architecture
[RndisDevices.NTia64]
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1042&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1045&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1052&MI_00
%RndisDevice_cust_1054%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1054&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1056&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1062&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1072&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1079&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1082&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10A6&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10AB&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10B2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C1&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10C5&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_10D2&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1203&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1231&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1BC7&PID_1251&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_2300&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1980&MI_00
%RndisDevice%    = RNDIS.NT.6.0, USB\VID_1bc7&PID_1982

;@@@ This is the common setting for setup
[ControlFlags]
ExcludeFromSelect=*

; DDInstall section
; References the in-build Netrndis.inf
[RNDIS.NT.6.0]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
; NEVER REMOVE THE FOLLOWING REFERENCE FOR NETRNDIS.INF
include         = netrndis.inf
needs           = usbrndis6.ndi
AddReg          = Rndis_AddReg
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD.
*MediaType         = 16   ; NdisMediumNative802_11
*PhysicalMediaType = 14   ; NdisPhysicalMedium802_3

; DDInstal.Services section
[RNDIS.NT.6.0.Services]
include     = netrndis.inf
needs       = usbrndis6.ndi.Services

; Optional registry settings. You can modify as needed.
[RNDIS_AddReg] 
HKR, NDI\params\RndisProperty, ParamDesc,  0, %Rndis_Property%
HKR, NDI\params\RndisProperty, type,       0, "edit"
HKR, NDI\params\RndisProperty, LimitText,  0, "12"
HKR, NDI\params\RndisProperty, UpperCase,  0, "1"
HKR, NDI\params\RndisProperty, default,    0, " "
HKR, NDI\params\RndisProperty, optional,   0, "1"

; No sys copyfiles - the sys files are already in-build 
; (part of the operating system).

; Modify these strings for your device as needed.
[Strings]
Microsoft             = "Telit"
RndisDevice           = "Telit Remote NDIS6"
RndisDevice_cust_1054 = "SKT T-Login Network Adapter(FT980-KS)"
Rndis_Property        = "Optional RNDIS Property"
