;
;   MUSBSer.INF (for Windows XP/Win7/Win8)
;
;   Copyright (c) 2011 - 2014, ASR Technology.

[version]
signature	= "$Windows NT$"
Class		= Ports
ClassGuid	= {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider	= %Pro%
DriverVer	= 11/12/2020, 2.0.0.9
CatalogFile	= musbser.cat


[ControlFlags]
;

[DestinationDirs]
DefaultDestDir=12
;ComPort.NT.Copy=12

[Manufacturer]
%Pro%=Pro, NTx86, NTamd64



;========================================= 32bit ==================================================
[Pro.NTx86]
;Add for ASR mobilephone product

%DeviceDesc% = ComPort, USB\VID_1bc7&PID_7010&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_7011&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_701A&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_701B&MI_03
;flashing,dump
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3004
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3004&MI_00
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3017
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3017&MI_00
%DeviceDesc_download% = ComPort, USB\VID_305A&PID_1415
%DeviceDesc_download% = ComPort, USB\VID_305A&PID_1415&MI_00
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9200
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9200&MI_00
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9201
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9201&MI_00

;========================================= 64bit ==================================================
[Pro.NTamd64]
;Add for ASR mobilephone product

%DeviceDesc% = ComPort, USB\VID_1bc7&PID_7010&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_7011&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_701A&MI_03
%DeviceDesc% = ComPort, USB\VID_1bc7&PID_701B&MI_03
;flashing,dump
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3004
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3004&MI_00
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3017
%DeviceDesc_download% = ComPort, USB\VID_2ECC&PID_3017&MI_00
%DeviceDesc_download% = ComPort, USB\VID_305A&PID_1415
%DeviceDesc_download% = ComPort, USB\VID_305A&PID_1415&MI_00
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9200
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9200&MI_00
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9201
%DeviceDesc_download% = ComPort, USB\VID_1BC7&PID_9201&MI_00


[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.Copy]
musbser.sys

[ComPort.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,musbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.AddReg]
HKR,"Parameters","DebugLevel",0x10001,5

[ComPort.NT.HW.AddReg]
;HKR,,"UpperFilters",0x00010000,"mfilter"

[ComPort.NT.Services]
AddService = MUSBSer, 0x00000002, Serial_Service_Inst

[Serial_Service_Inst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 1               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\MUSBSer.sys
AddReg         = ComPort.AddReg
LoadOrderGroup = Base

[SourceDisksNames.x86]
1 = %Pro.Disk%,Disk1,,\MUSBSer\i386

[SourceDisksNames.amd64]
1 = %Pro.Disk%,Disk1,,\MUSBSer\amd64

[SourceDisksFiles]
musbser.sys = 1

[Strings]
Pro 			= "Telit"
Pro.Disk		= "Telit AT Interface Installation Disk"
Serial.SVCDESC  = "AT Interface driver"
; ACM device name on single CP DKB or WB(TTC) ACM device name On DSDT DKB
DeviceDesc 		= "Telit Serial Device"
DeviceDesc_download = "ASR Serial Download Device"
