comment;			BRIDGETOWN AUTO-CONFIGURATION MAPPINGS

comment; Configure the duplex unit by querying the SysObject ID to the device.
ACF_SEQUENCE_CONTAINS;installable-duplex-unit-actual;1.3.6.1.2.1.1.2;

1.3.6.1.4.1.253.8.62.1.19.4.37.1.1;not-installed
1.3.6.1.4.1.253.8.62.1.19.4.37.2.1;installed
1.3.6.1.4.1.253.8.62.1.20.6.34.2.1;installed
1.3.6.1.4.1.253.8.62.1.20.6.34.1.1;not-installed

end;

comment; Feature Set is based on the sysobject ID
ACF_SEQUENCE_CONTAINS;installable-phaser-module-actual;1.3.6.1.2.1.1.2;
	1.3.6.1.4.1.253.8.62.1.20.6.34.2.1;dn	
	1.3.6.1.4.1.253.8.62.1.19.4.37.1.1;n
	1.3.6.1.4.1.253.8.62.1.19.4.37.2.1;dn
	1.3.6.1.4.1.253.8.62.1.20.6.34.1.1;n
	
	model-default;Xerox Phaser 6600N;n
	model-default;Xerox Phaser 6600DN;dn
	model-default;Xerox WorkCentre 6605N;n	
	model-default;Xerox WorkCentre 6605DN;dn
end;

comment; Tray configurations is a SequenceContaining type of feature.  Basically, we see if the required oid is present.
ACF_SEQUENCE_CONTAINS_OID;installable-input-paper-trays-actual;1.3.6.1.2.1.43.8.2.1.13;
	1.3.6.1.2.1.43.8.2.1.13.1.3;3-trays;
	default;2-trays
	end;

comment; Job Storage 
ACF_VALUE_EQUALS_MAP;installable-job-storage-actual;1.3.6.1.2.1.25.2.3.1.2.2;
	1.3.6.1.2.1.25.2.1.5;hard-drive;
	1.3.6.1.2.1.25.2.1.8;ram-disk;
 	default;not-installed
	model-default;Xerox Phaser 6600N;not-installed
	model-default;Xerox Phaser 6600DN;not-installed
	model-default;Xerox WorkCentre 6605N;ram-disk
	model-default;Xerox WorkCentre 6605DN;ram-disk
 	end;	

	
comment; LanFax
comment; This is assumed to always be the 15th service index, and the way it has been detcted in the past is by checking the
comment; xcmSvcMonServiceStateDetail.  However, this is always returned as a HEX_STRING, which is actually representing
comment; a bitmask.  It is a 6 character hex string, where each character represents 8 bits for 48-bit flags.  A string of
comment; "00 00 00 00 00 80" is actually akin to "0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 1000 0000", where the 40th bit is set.  
comment; When looking at this feature in the device profile (MIB Spec), you will note that it referrs to bits representing states.  For this
comment; feature, we will mark it as installed if bits 40, 41, or 42 are set, otherwise it will be marked as not installed.
ACF_VALUE_EQUALS_MAP;installable-fax-out-actual;1.3.6.1.4.1.253.8.74.5.2.1.16.15;
	00 00 00 00 00 80;installed;
	00 00 00 00 00 40;installed;
	00 00 00 00 00 20;installed;
	default;not-installed
end;

comment; LANFax is based on the sysobject ID
ACF_VALUE_EQUALS_MAP;installable-fax-out-actual;1.3.6.1.2.1.1.2.0;
	1.3.6.1.4.1.253.8.62.1.20.6.34.1.1;installed
	1.3.6.1.4.1.253.8.62.1.20.6.34.2.1;installed
	default;not-installed
	model-default;Xerox WorkCentre 6605N;installed
	model-default;Xerox Phaser 6600N;not-installed
	model-default;Xerox Phaser 6600DN;not-installed	
	model-default;Xerox WorkCentre 6605DN;installed
	end;
