; yk51x86.inf created 01-Apr-2005
;
; Marvell Yukon Ethernet Controller 
;
; (C)Copyright 2002-2005 Marvell(R).
; 
; All rights reserved.
;
; INF File for NDIS5.1 Miniport Driver for Windows XP and Server 2003 (x86) YK51X86.sys v8.25.1.3

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %Marvell%
CatalogFile	= yk51x86.CAT
DriverVer=04/01/2005, 8.25.1.3

[Manufacturer]


%Marvell%	= Marvell, NT.5.1, NT.5.2



[ControlFlags]

ExcludeFromSelect	= *


;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[Marvell]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP
;
;-----------------------------------------------------------------------------
[Marvell.NT.5.1]

%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_952111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_502111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_012111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_032111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_102111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_811A1043
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_173C1043
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_80011019
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0F381019
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00851025
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_004715D4
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1406147B
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_E0001458
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_90251695
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0C19105B
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1C0317F2
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_2803270F

%Yukon.DeviceDesc4340% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4340&SUBSYS_212111AB

%Yukon.DeviceDesc4341% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_222211AB
%Yukon.DeviceDesc4341% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_3015107B

%Yukon.DeviceDesc4342% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4342&SUBSYS_612111AB

%Yukon.DeviceDesc4343% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_622211AB
%Yukon.DeviceDesc4343% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_3015107B

%Yukon.DeviceDesc4344SX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_218111AB
%Yukon.DeviceDesc4344LX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_219111AB

%Yukon.DeviceDesc4345SX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_228211AB
%Yukon.DeviceDesc4345LX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_229211AB

%Yukon.DeviceDesc4346SX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_618111AB
%Yukon.DeviceDesc4346LX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_619111AB

%Yukon.DeviceDesc4347SX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_628211AB
%Yukon.DeviceDesc4347LX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_629211AB

%Yukon.DeviceDesc4350% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_352111AB
%Yukon.DeviceDesc4350% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00BA11AB
%Yukon.DeviceDesc4350% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00011179

%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_362111AB
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00BA11AB
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00011179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF101179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000D1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000E1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000F1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00111854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00121854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00141854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00151854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00161854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00171854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00181854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001A1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001C1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001E1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001B1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00201854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00211854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00221854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00231854
%Yukon.DeviceDesc4351% = SLYuk2CopFastGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4009107B
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF001179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_203D161F
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0506107B
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_AC1213D1
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_833810F7
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0733152D
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0300107B
%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_11111071
%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_902B1695

%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_522111AB
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_81341043
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_052C1462
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001458
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001940
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00871025
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00861025
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_80521849
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0509A0A0
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4009107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3031107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3032107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5052107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5053107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B

%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_502111AB
%Yukon.DeviceDesc4361% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3015107B
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_50218086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_30638086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34528086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34538086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34608086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34618086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34648086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34658086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34628086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34638086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343D8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343E8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34398086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343A8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343B8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343C8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345A8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34588086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34598086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345B8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345E8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345F8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345C8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345D8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34508086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34518086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34668086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34678086

%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_532111AB
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00BA11AB
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81421043
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2A0D103C
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058C1462
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001458
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001940
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_90291695
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_100315BD
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506A0A0
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2C0817F2
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_A43010FD
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531849
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00011179
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF101179
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2801270F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_04A01558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000B1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000C1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00101854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00131854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00191854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001F1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001D1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00241854
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3197109F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058517FF
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0733152D
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatGw.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0300107B
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF001179
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001214C0
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203C161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203D161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204A161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatGw.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506107B
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2401297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2411297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2421297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2431297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2441297
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AC1113D1
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_833810F7
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_01111071
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_10B717C0
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05901558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05911558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05921558

%SK-9872.DeviceDesc%	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98721148
%SK-9871-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50711148
%SK-9871.DeviceDesc%       = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98711148
%SK-9862.DeviceDesc%    	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98621148
%SK-9861-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50611148
%SK-9861.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98611148
%SK-9851-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50511148
%SK-9844.DeviceDesc%    	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98441148
%SK-9843-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50431148
%SK-9843.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98431148
%SK-9842.DeviceDesc%	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98421148
%SK-9841-V2.DeviceDesc% = SlYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50411148
%SK-9841.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98411148
%SK-9822.DeviceDesc%    	 = DLGenCopGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98221148
%SK-9821-V2.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50211148
%SK-9821.DeviceDesc%    	 = SLGenCopGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98211148
%SK-9521.DeviceDesc%    	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_95211148
%SK-9521-V2.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_32211148
%RDK-8012.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_12211148
%RDK-8011.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_11211148
%RDK-8009.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_09211148
%RDK-8008.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_08211148
%RDK-8007.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_07211148
%RDK-8006.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_06211148
%RDK-8004.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_04211148
%RDK-8003.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_03211148
%RDK-8002.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_02211148
%RDK-8001.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_01211148
%SK-9E21.DeviceDesc%    	 = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148


%SKYukon.DeviceDesc9E21D% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148
%SKYukon.DeviceDesc9E21% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21001148
%SKYukon.DeviceDesc9E22% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22001148
%SKYukon.DeviceDesc9E81% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_81001148
%SKYukon.DeviceDesc9E82% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_82001148
%SKYukon.DeviceDesc9E91% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_91001148
%SKYukon.DeviceDesc9E92% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_92001148

%SKYukon.DeviceDesc9S21% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_21001148
%SKYukon.DeviceDesc9S22% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22001148
%SKYukon.DeviceDesc9S81% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_81001148
%SKYukon.DeviceDesc9S82% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82001148
%SKYukon.DeviceDesc9S91% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_91001148
%SKYukon.DeviceDesc9S92% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_92001148 

%Yukon.DeviceDescGen% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4340
%Yukon.DeviceDescGen% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4342
%Yukon.DeviceDescGen% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347 
%Yukon.DeviceDescGen% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4350
%Yukon.DeviceDescGen% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362


;-----------------------------------------------------------------------------
;
;       Windows Server 2003
;
;-----------------------------------------------------------------------------
[Marvell.NT.5.2]

%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_952111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_502111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_012111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_032111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_102111AB
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_811A1043
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_173C1043
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_80011019
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0F381019
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_00851025
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_004715D4
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1406147B
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_E0001458
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_90251695
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_0C19105B
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_1C0317F2
%Yukon.DeviceDesc4320% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_2803270F

%Yukon.DeviceDesc4340% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4340&SUBSYS_212111AB

%Yukon.DeviceDesc4341% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_222211AB
%Yukon.DeviceDesc4341% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341&SUBSYS_3015107B

%Yukon.DeviceDesc4342% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4342&SUBSYS_612111AB

%Yukon.DeviceDesc4343% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_622211AB
%Yukon.DeviceDesc4343% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343&SUBSYS_3015107B

%Yukon.DeviceDesc4344SX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_218111AB
%Yukon.DeviceDesc4344LX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344&SUBSYS_219111AB

%Yukon.DeviceDesc4345SX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_228211AB
%Yukon.DeviceDesc4345LX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345&SUBSYS_229211AB

%Yukon.DeviceDesc4346SX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_618111AB
%Yukon.DeviceDesc4346LX% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346&SUBSYS_619111AB

%Yukon.DeviceDesc4347SX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_628211AB
%Yukon.DeviceDesc4347LX% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347&SUBSYS_629211AB

%Yukon.DeviceDesc4350% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_352111AB
%Yukon.DeviceDesc4350% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00BA11AB
%Yukon.DeviceDesc4350% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4350&SUBSYS_00011179

%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_362111AB
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00BA11AB
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00011179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF101179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000D1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000E1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_000F1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00111854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00121854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00141854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00151854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00161854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00171854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00181854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001A1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001C1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001E1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_001B1854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00201854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00211854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00221854
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatLg.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_00231854
%Yukon.DeviceDesc4351% = SLYuk2CopFastGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_4009107B
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatTo.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_FF001179
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_203D161F
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0506107B
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_AC1213D1
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_833810F7
%Yukon.DeviceDesc4351% = SLYuk2CopFastBat.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0733152D
%Yukon.DeviceDesc4351% = SLYuk2CopFastBatGw.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_0300107B
%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_11111071
%Yukon.DeviceDesc4351% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351&SUBSYS_902B1695

%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_522111AB
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_81341043
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_052C1462
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001458
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_E0001940
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00871025
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_00861025
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_80521849
%Yukon.DeviceDesc4360% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_0509A0A0
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4009107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3031107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_3032107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5052107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_5053107B
%Yukon.DeviceDesc4360% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4360&SUBSYS_4039107B

%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_502111AB
%Yukon.DeviceDesc4361% = SLYuk2CopGigGw.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_3015107B
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_50218086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_30638086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34528086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34538086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34608086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34618086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34648086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34658086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34628086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34638086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343D8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343E8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34398086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343A8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343B8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_343C8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345A8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34588086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34598086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345B8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345E8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345F8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345C8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_345D8086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34508086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34518086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34668086
%Yukon.DeviceDesc4361% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361&SUBSYS_34678086

%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_532111AB
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00BA11AB
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_81421043
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2A0D103C
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058C1462
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001458
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_E0001940
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_90291695
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_100315BD
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506A0A0
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2C0817F2
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_A43010FD
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_80531849
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00011179
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF101179
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_2801270F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_04A01558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000B1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_000C1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00101854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00131854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00191854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001F1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001D1854
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatLg.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_00241854
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_3197109F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_058517FF
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0733152D
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatGw.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0300107B
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatTo.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_FF001179
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_001214C0
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203C161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_203D161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_204A161F
%Yukon.DeviceDesc4362% = SLYuk2CopGigBatGw.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_0506107B
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2401297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2411297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2421297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2431297
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_C2441297
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_AC1113D1
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_833810F7
%Yukon.DeviceDesc4362% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_01111071
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_10B717C0
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05901558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05911558
%Yukon.DeviceDesc4362% = SLYuk2CopGigBat.ndi, PCI\VEN_11AB&DEV_4362&SUBSYS_05921558

%SK-9872.DeviceDesc%	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98721148
%SK-9871-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50711148
%SK-9871.DeviceDesc%       = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98711148
%SK-9862.DeviceDesc%    	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98621148
%SK-9861-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50611148
%SK-9861.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98611148
%SK-9851-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50511148
%SK-9844.DeviceDesc%    	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98441148
%SK-9843-V2.DeviceDesc% = SLYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50431148
%SK-9843.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98431148
%SK-9842.DeviceDesc%	 = DLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98421148
%SK-9841-V2.DeviceDesc% = SlYukFibGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50411148
%SK-9841.DeviceDesc%    	 = SLGenFibGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98411148
%SK-9822.DeviceDesc%    	 = DLGenCopGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98221148
%SK-9821-V2.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_50211148
%SK-9821.DeviceDesc%    	 = SLGenCopGig.ndi, PCI\VEN_1148&DEV_4300&SUBSYS_98211148
%SK-9521.DeviceDesc%    	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_95211148
%SK-9521-V2.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_32211148
%RDK-8012.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_12211148
%RDK-8011.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_11211148
%RDK-8009.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_09211148
%RDK-8008.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_08211148
%RDK-8007.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_07211148
%RDK-8006.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_06211148
%RDK-8004.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_04211148
%RDK-8003.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_03211148
%RDK-8002.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_02211148
%RDK-8001.DeviceDesc%   	 = SLYukCopGig.ndi, PCI\VEN_1148&DEV_4320&SUBSYS_01211148
%SK-9E21.DeviceDesc%    	 = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148


%SKYukon.DeviceDesc9E21D% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21D01148
%SKYukon.DeviceDesc9E21% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_21001148
%SKYukon.DeviceDesc9E22% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_22001148
%SKYukon.DeviceDesc9E81% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_81001148
%SKYukon.DeviceDesc9E82% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_82001148
%SKYukon.DeviceDesc9E91% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_91001148
%SKYukon.DeviceDesc9E92% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9E00&SUBSYS_92001148

%SKYukon.DeviceDesc9S21% = SLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_21001148
%SKYukon.DeviceDesc9S22% = DLYuk2CopGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_22001148
%SKYukon.DeviceDesc9S81% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_81001148
%SKYukon.DeviceDesc9S82% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_82001148
%SKYukon.DeviceDesc9S91% = SLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_91001148
%SKYukon.DeviceDesc9S92% = DLYuk2FibGig.ndi, PCI\VEN_1148&DEV_9000&SUBSYS_92001148 

%Yukon.DeviceDescGen% = SLYukCopGig.ndi, PCI\VEN_11AB&DEV_4320
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4340
%Yukon.DeviceDescGen% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4341
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4342
%Yukon.DeviceDescGen% = DLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4343
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4344
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4345
%Yukon.DeviceDescGen% = SLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4346
%Yukon.DeviceDescGen% = DLYuk2FibGig.ndi, PCI\VEN_11AB&DEV_4347 
%Yukon.DeviceDescGen% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4350
%Yukon.DeviceDescGen% = SLYuk2CopFast.ndi, PCI\VEN_11AB&DEV_4351
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4360
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4361
%Yukon.DeviceDescGen% = SLYuk2CopGig.ndi, PCI\VEN_11AB&DEV_4362




;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link>

[SLGenFibGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.TxRxBuff.params, yk51x86.GigFrSize.params,
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLGenFibGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link>

[SLGenCopGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.TxRxBuff.params, yk51x86.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLGenCopGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <dual link>

[DLGenFibGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.TxRxBuff.params, yk51x86.DualLink.params, yk51x86.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[DLGenFibGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <dual link> Copper Adapters

[DLGenCopGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params,  yk51x86.TxRxBuff.params, yk51x86.DualLink.params, yk51x86.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[DLGenCopGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Version 2.0 Copper>

[SLYukCopGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxBuff.params, yk51x86.WoL.params, yk51x86.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYukCopGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Version 2.0 Copper>

[SLYukFibGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.TxRxBuff.params, yk51x86.GigFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYukFibGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Copper>

[SLYuk2CopGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.WoL.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Copper>

[SLYuk2CopGigGw.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.WoL.params.Gw, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGigGw.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Fiber>

[SLYuk2FibGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.TxRxLE.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2FibGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version>

[SLYuk2CopFast.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.WoL.params, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFast.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version>

[SLYuk2CopFastGw.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.WoL.params.Gw, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFastGw.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <copper single link> with battery support

[SLYuk2CopGigBat.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGigBat.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <copper single link> with battery support

[SLYuk2CopGigBatGw.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params.Gw, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGigBatGw.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <copper single link> with battery support

[SLYuk2CopGigBatLg.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params.Lg, yk51x86.WoL.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGigBatLg.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version> with battery support

[SLYuk2CopFastBat.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFastBat.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version> with battery support

[SLYuk2CopFastBatGw.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params.Gw, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFastBatGw.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version> with battery support special case

[SLYuk2CopFastBatLg.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params.Lg, yk51x86.WoL.params, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFastBatLg.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <copper single link> with battery support

[SLYuk2CopGigBatTo.ndi]
DelReg= yk51x86.delreg
DelReg= yk51x86.delreg.To
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params.To, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopGigBatTo.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; 10/100 FastEthernet Adapters <single link Version> with battery support

[SLYuk2CopFastBatTo.ndi]
DelReg= yk51x86.delreg
DelReg= yk51x86.delreg.To
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.SingleLink.params, yk51x86.SLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.Bat.params, yk51x86.WoL.params.To, yk51x86.TcpSegm.params, yk51x86.FastFrSize.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[SLYuk2CopFastBatTo.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <dual link>

[DLYuk2FibGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params,  yk51x86.TxRxLE.params, yk51x86.DualLink.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[DLYuk2FibGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog

;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <dual link> Copper Adapters

[DLYuk2CopGig.ndi]
DelReg= yk51x86.delreg
AddReg		= yk51x86.reg, yk51x86.params, yk51x86.DLSpeedDuplex.params, yk51x86.TxRxLE.params, yk51x86.DualLink.params, yk51x86.GigFrSize.params, yk51x86.TcpSegm.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= yk51x86.CopyFiles

[DLYuk2CopGig.ndi.Services]
DelService = yukon, 204
DelService = sk98wxp, 204
AddService	= yukonwxp, 2, yukonwxp.Service, common.EventLog


;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[yk51x86.params]

HKR, Ndi\Params\HwChecksum,		ParamDesc,	0, %HwCsum%
HKR, Ndi\Params\HwChecksum,		Type,		0, "enum"
HKR, Ndi\Params\HwChecksum\enum,	"1",			0, %On%
HKR, Ndi\Params\HwChecksum\enum,	"0",			0, %Off%
HKR, Ndi\Params\HwChecksum,		Default,		0, "1"

HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %LogMsg%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\Moderate,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\Moderate,		Type,		0, "enum"
HKR, Ndi\Params\Moderate\enum,	"1",			0, %On%
HKR, Ndi\Params\Moderate\enum,	"0",			0, %Off%
HKR, Ndi\Params\Moderate,		Default,		0, "1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"


;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[yk51x86.TxRxBuff.params]



HKR, Ndi\Params\MaxReceives,	ParamDesc,	0, %NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,		0, "int"
HKR, Ndi\Params\MaxReceives,	Base,		0, "10"
HKR, Ndi\Params\MaxReceives,	Min,			0, "3"
HKR, Ndi\Params\MaxReceives,	Max,			0, "500"
HKR, Ndi\Params\MaxReceives,	Step,		0, "1"
HKR, Ndi\Params\MaxReceives,	Default,		0, "50"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,	0, %NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,		0, "int"
HKR, Ndi\Params\MaxTransmits,	Base,		0, "10"
HKR, Ndi\Params\MaxTransmits,	Min,			0, "4"
HKR, Ndi\Params\MaxTransmits,	Max,			0, "200"
HKR, Ndi\Params\MaxTransmits,	Step,		0, "1"
HKR, Ndi\Params\MaxTransmits,	Default,		0, "50"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[yk51x86.TxRxLE.params]


HKR, Ndi\Params\MaxReceives,	ParamDesc,	0, %NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,		0, "int"
HKR, Ndi\Params\MaxReceives,	Base,		0, "10"
HKR, Ndi\Params\MaxReceives,	Min,			0, "256"
HKR, Ndi\Params\MaxReceives,	Max,			0, "512"
HKR, Ndi\Params\MaxReceives,	Step,		0, "128"
HKR, Ndi\Params\MaxReceives,	Default,		0, "256"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,	0, %NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,		0, "int"
HKR, Ndi\Params\MaxTransmits,	Base,		0, "10"
HKR, Ndi\Params\MaxTransmits,	Min,			0, "256"
HKR, Ndi\Params\MaxTransmits,	Max,			0, "512"
HKR, Ndi\Params\MaxTransmits,	Step,		0, "128"
HKR, Ndi\Params\MaxTransmits,	Default,		0, "256"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[yk51x86.GigFrSize.params]


HKR, Ndi\Params\MaxFrameSize,           ParamDesc,      0, %MaxFrSize%
HKR, Ndi\Params\MaxFrameSize,           default,        0, "1514"
HKR, Ndi\Params\MaxFrameSize\Enum,      "1514",         0, %Disabled%
HKR, Ndi\Params\MaxFrameSize\Enum,      "4088",         0, %Bytes4088%
HKR, Ndi\Params\MaxFrameSize\Enum,      "9014",         0, %Bytes9014%
HKR, Ndi\Params\MaxFrameSize,           type,           0, "enum"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100 chip)
;
;-----------------------------------------------------------------------------
[yk51x86.FastFrSize.params]

HKR,, MaxFrameSize,, "1514"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk51x86.Bat.params]


HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",			0, %Fast%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",			0, %Gig%
HKR, Ndi\Params\BatterySpeedSettings,		Default,		0, "4"

HKR, Ndi\Params\BatteryModeLinkDetection,		ParamDesc,	0, %BatLinkDet%
HKR, Ndi\Params\BatteryModeLinkDetection,		Type,		0, "enum"
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"0",			0, %NoPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"1",			0, %MaxPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"4",			0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection,		Default,		0, "4"

HKR,, BatteryPowerCheckInterval,, "20"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for battery powered Adapters
;
;-----------------------------------------------------------------------------
[yk51x86.Bat.params.Lg]


HKR, Ndi\Params\BatterySpeedSettings,		ParamDesc,	0, %BatSpeed%
HKR, Ndi\Params\BatterySpeedSettings,		Type,		0, "enum"
HKR, Ndi\Params\BatterySpeedSettings\enum,	"3",			0, %Fast%
HKR, Ndi\Params\BatterySpeedSettings\enum,	"4",			0, %Gig%
HKR, Ndi\Params\BatterySpeedSettings,		Default,		0, "3"

HKR, Ndi\Params\BatteryModeLinkDetection,		ParamDesc,	0, %BatLinkDet%
HKR, Ndi\Params\BatteryModeLinkDetection,		Type,		0, "enum"
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"0",			0, %NoPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"1",			0, %MaxPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection\enum,	"4",			0, %EnDetPwrSave%
HKR, Ndi\Params\BatteryModeLinkDetection,		Default,		0, "1"



;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[yk51x86.WoL.params]


HKR, Ndi\Params\WakeUpModeCap_A,			ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,			Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",			0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",			0, %Magic Packet%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",			0, %Pattern Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",			0, %Mag Pack Patt Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"28",			0, %Link Change%
HKR, Ndi\Params\WakeUpModeCap_A,			Default,		0, "27"

HKR, Ndi\Params\WakeFromShutdown,			ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,			Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",			0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",			0, %Off%
HKR, Ndi\Params\WakeFromShutdown,			Default,		0, "0"


;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan for To notebooks
;
;-----------------------------------------------------------------------------
[yk51x86.WoL.params.To]


HKR, Ndi\Params\WakeUpModeCap_A,			ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,			Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",			0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",			0, %Magic Packet%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",			0, %Pattern Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",			0, %Mag Pack Patt Match%
HKR, Ndi\Params\WakeUpModeCap_A,			Default,		0, "27"

HKR, Ndi\Params\WakeFromShutdown,			ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,			Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",			0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",			0, %Off%
HKR, Ndi\Params\WakeFromShutdown,			Default,		0, "0"



;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan for To notebooks
;
;-----------------------------------------------------------------------------
[yk51x86.WoL.params.Gw]


HKR, Ndi\Params\WakeUpModeCap_A,			ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,			Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",			0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",			0, %Magic Packet%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",			0, %Pattern Match%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",			0, %Mag Pack Patt Match%
HKR, Ndi\Params\WakeUpModeCap_A,			Default,		0, "25"

HKR, Ndi\Params\WakeFromShutdown,			ParamDesc,	0, %WakeFromShut%
HKR, Ndi\Params\WakeFromShutdown,			Type,		0, "enum"
HKR, Ndi\Params\WakeFromShutdown\enum,	"1",			0, %On%
HKR, Ndi\Params\WakeFromShutdown\enum,	"0",			0, %Off%
HKR, Ndi\Params\WakeFromShutdown,			Default,		0, "1"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[yk51x86.TcpSegm.params]

HKR, Ndi\Params\TcpLargeSend,		ParamDesc,	0, %TcpSegmentation%
HKR, Ndi\Params\TcpLargeSend,		Type,		0, "enum"
HKR, Ndi\Params\TcpLargeSend\enum,	"1",			0, %Enabled%
HKR, Ndi\Params\TcpLargeSend\enum,	"0",			0, %Disabled%
HKR, Ndi\Params\TcpLargeSend,		Default,		0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[yk51x86.SingleLink.params]

HKR, Ndi\Params\TagHeaderSupport_A,		ParamDesc,	0, %QoSSup%
HKR, Ndi\Params\TagHeaderSupport_A,		Type,		0, "enum"
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"1",			0, %On%
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"0",			0, %Off%
HKR, Ndi\Params\TagHeaderSupport_A,		Default,		0, "0"

HKR, Ndi\Params\FlowControl_A,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\FlowControl_A,		Type,		0, "enum"
HKR, Ndi\Params\FlowControl_A\enum,	"3",			0, %On%
HKR, Ndi\Params\FlowControl_A\enum,	"0",			0, %Off%
HKR, Ndi\Params\FlowControl_A,		Default,		0, "3"



HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[yk51x86.SLSpeedDuplex.params]


HKR,Ndi\Params\ConnectionType_A,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\ConnectionType_A,      Type,       0, "enum"
HKR,Ndi\Params\ConnectionType_A,      Default,    0, "0"
HKR,Ndi\Params\ConnectionType_A\enum, "0",        0, %Autosense%
HKR,Ndi\Params\ConnectionType_A\enum, "1",        0, %10MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "2",        0, %10MFD%
HKR,Ndi\Params\ConnectionType_A\enum, "3",        0, %100MHD%
HKR,Ndi\Params\ConnectionType_A\enum, "4",        0, %100MFD%

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Dual Link Adapters
;
;-----------------------------------------------------------------------------
[yk51x86.DualLink.params]

HKR, Ndi\Params\TagHeaderSupport_A,		ParamDesc,	0, %QoSSupA%
HKR, Ndi\Params\TagHeaderSupport_A,		Type,		0, "enum"
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"1",			0, %On%
HKR, Ndi\Params\TagHeaderSupport_A\enum,	"0",			0, %Off%
HKR, Ndi\Params\TagHeaderSupport_A,		Default,		0, "0"

HKR, Ndi\Params\TagHeaderSupport_B,		ParamDesc,	0, %QoSSupB%
HKR, Ndi\Params\TagHeaderSupport_B,		Type,		0, "enum"
HKR, Ndi\Params\TagHeaderSupport_B\enum,	"1",			0, %On%
HKR, Ndi\Params\TagHeaderSupport_B\enum,	"0",			0, %Off%
HKR, Ndi\Params\TagHeaderSupport_B,		Default,		0, "0"


HKR, Ndi\Params\RlmtMode,		ParamDesc,	0, %RLMT%
HKR, Ndi\Params\RlmtMode,		Type,		0, "enum"
HKR, Ndi\Params\RlmtMode\enum,	"1",			0, %Link%
HKR, Ndi\Params\RlmtMode\enum,	"3",			0, %OtherPort%
HKR, Ndi\Params\RlmtMode\enum,	"7",			0, %Segment%
HKR, Ndi\Params\RlmtMode,		Default,		0, "1"

HKR, Ndi\Params\PreferredPort,		ParamDesc,	0, %Preferred%
HKR, Ndi\Params\PreferredPort,		Type,		0, "enum"
HKR, Ndi\Params\PreferredPort\enum,	"1",			0, %A%
HKR, Ndi\Params\PreferredPort\enum,	"2",			0, %B%
HKR, Ndi\Params\PreferredPort,		Default,		0, "1"

;Port A Parameters
;---------------
HKR, Ndi\Params\FlowControl_A,		ParamDesc,		0, %FlowCtrlA%
HKR, Ndi\Params\FlowControl_A,		Type,			0, "enum"
HKR, Ndi\Params\FlowControl_A\enum,	"3",				0, %On%
HKR, Ndi\Params\FlowControl_A\enum,	"0",				0, %Off%
HKR, Ndi\Params\FlowControl_A,		Default,			0, "3"

;Port B Parameters
;---------------
HKR, Ndi\Params\FlowControl_B,		ParamDesc,		0, %FlowCtrlB%
HKR, Ndi\Params\FlowControl_B,		Type,			0, "enum"
HKR, Ndi\Params\FlowControl_B\enum,	"3",				0, %On%
HKR, Ndi\Params\FlowControl_B\enum,	"0",				0, %Off%
HKR, Ndi\Params\FlowControl_B,		Default,			0, "3"


HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"
HKR,, RlmtChgBCPrio,, "0"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[yk51x86.DLSpeedDuplex.params]


;Port A Parameters
;---------------
HKR,Ndi\Params\ConnectionType_A,		ParamDesc,	0, %SpeedDuplexA%
HKR,Ndi\Params\ConnectionType_A,		Type,		0, "enum"
HKR,Ndi\Params\ConnectionType_A,		Default,		0, "0"
HKR,Ndi\Params\ConnectionType_A\enum,	"0",			0, %Autosense%
HKR,Ndi\Params\ConnectionType_A\enum,	"1",			0, %10MHD%
HKR,Ndi\Params\ConnectionType_A\enum,	"2",			0, %10MFD%
HKR,Ndi\Params\ConnectionType_A\enum,	"3",			0, %100MHD%
HKR,Ndi\Params\ConnectionType_A\enum,	"4",			0, %100MFD%


;Port B Parameters
;---------------
HKR,Ndi\Params\ConnectionType_B,		ParamDesc,	0, %SpeedDuplexB%
HKR,Ndi\Params\ConnectionType_B,		Type,		0, "enum"
HKR,Ndi\Params\ConnectionType_B,		Default,		0, "0"
HKR,Ndi\Params\ConnectionType_B\enum,	"0",			0, %Autosense%
HKR,Ndi\Params\ConnectionType_B\enum,	"1",			0, %10MHD%
HKR,Ndi\Params\ConnectionType_B\enum,	"2",			0, %10MFD%
HKR,Ndi\Params\ConnectionType_B\enum,	"3",			0, %100MHD%
HKR,Ndi\Params\ConnectionType_B\enum,	"4",			0, %100MFD%


;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[yk51x86.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "yukonwxp"


;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys 
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[yk51x86.delreg]
; remove the "OS Controlled" (15) subkey from WakeUpModeCap_X
HKR, Ndi\Params\WakeUpModeCap_A\enum,15
HKR, Ndi\Params\WakeUpModeCap_B\enum,15
HKR, Ndi\Params\DuplexCapabilities_A
HKR, Ndi\Params\DuplexCapabilities_B
HKR, Ndi\Params\FlowControl_A
HKR, Ndi\Params\FlowControl_B
HKR, Ndi\Params\AutoNegotiation_A
HKR, Ndi\Params\AutoNegotiation_B
HKR, Ndi\Params\Role_A
HKR, Ndi\Params\Role_B
HKR, Ndi\Params\Speed_A
HKR, Ndi\Params\Speed_B
HKR, Ndi\Params\MaxFrameSize

;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys 
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[yk51x86.delreg.To]
; remove the "Link Change" (28) subkey from WakeUpModeCap_X
HKR, Ndi\Params\WakeUpModeCap_A\enum,28

;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[yukonwxp.Service]
DisplayName	= %yk51x86.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\yk51x86.sys
LoadOrderGroup = NDIS


;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\yk51x86.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
yk51x86.sys	= 1,,

[yk51x86.CopyFiles]
yk51x86.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
yk51x86.CopyFiles	= 12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Network Address"
HwCsum = "Hardware Checksumming"
WakeUpCaps   = "Wake Up Capabilities"
IntMod = "Interrupt Moderation"
MaxIrq = "Max IRQ per Sec"
LogMsg = "Log Status Messages"
NumRcv = "Number of Receive Buffers"
NumTx  = "Number of Transmit Buffers"
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferred Port"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
A = "A"
B = "B"
Slave = "Slave"
Master = "Master"
Auto = "Auto"
both = "Half and Full Duplex"
full = "Full Duplex"
half = "Half Duplex"
bothFC = "Asymmetrical and Symmetrical Flow Control"
sym = "Symmetrical Flow Control"
asym = "Asymmetrical Flow Control"
noFc = "No Flow Control"
Autosense = "Auto-Sense"
10MHD = "10Mbps Half Duplex"
10MFD = "10Mbps Full Duplex"
100MHD = "100Mbps Half Duplex"
100MFD = "100Mbps Full Duplex"
Magic Packet = "Magic Packet"
Pattern Match = "Pattern Match"
Mag Pack Patt Match = "Magic Packet and Pattern Match"
Link Change = "Link Change"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
FlowCtrl = "FlowControl"
FlowCtrlA = "FlowControl Port A"
FlowCtrlB = "FlowControl Port B"
QoSSup = "802.1p Support"
QoSSupA = "802.1p Support Port A"
QoSSupB = "802.1p Support Port B"
WakeFromShut = "Wake From Shutdown"
TcpSegmentation = "TCP Segmentation"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;-----------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"

Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


;-----------------------------------------------------------------------------

; Chinese (Taiwan)
[Strings.0404]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "網路位址"
HwCsum = "硬體檢查總和"
WakeUpCaps   = "喚醒功能"
IntMod = "中断模式"
MaxIrq = "最大 IRQ数量"
LogMsg = "日誌狀態訊息"
NumRcv = "接收緩衝區數量"
NumTx  = "傳輸緩衝區數量"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "偏好埠"
On = "開啟"
Off = "關閉"
Non = "無"
Err = "錯誤"
Wrn = "警告"
Sta = "狀態訊息"
All = "所有訊息"
A = "A"
B = "B"
QoSSupA = "802.1p 支援 埠 A"
QoSSupB = "802.1p 支援 埠 B"
Slave = "从属"
Master = "主控"
Auto = "自動"
both = "半雙工兼全雙工"
full = "全雙工"
half = "半雙工"
FlowCtrlA = "流量控制 埠 A"
FlowCtrlB = "流量控制 埠 B"
bothFC = "不對稱和對稱流量控制"
sym = "對稱流量控制"
asym = "不對稱流量控制"
noFc = "無流量控制"
Autosense = "自動感應"
10MHD = "10Mbps 半雙工"
10MFD = "10Mbps 全雙工"
100MHD = "100Mbps 半雙工"
100MFD = "100Mbps 全雙工"
Magic Packet = "Magic Packet唤醒模式"
Pattern Match = "Pattern Match唤醒模式"
Mag Pack Patt Match = "Magic Packet 和Pattern Match唤醒模式"
Link Change = "Link Change唤醒模式"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "网络地址"
HwCsum = "硬件检查和"
WakeUpCaps   = "唤醒功能"
IntMod = "中断模式"
MaxIrq = "最大 IRQ数量"
LogMsg = "日志状态信息"
NumRcv = "接收缓存区数量"
NumTx  = "传送缓存区数量"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "首选端口"
On = "开"
Off = "关"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
A = "A"
B = "B"
QoSSupA = "802.1p 支持端口 A"
QoSSupB = "802.1p 支持端口 B"
Slave = "从属"
Master = "主控"
Auto = "自动"
both = "半双工兼全双工"
full = "全双工"
half = "半双工"
FlowCtrlA = "流控制端口 A"
FlowCtrlB = "流控制端口 B"
bothFC = "不对称和对称流控制"
sym = "对称流控制"
asym = "不对称流控制"
noFc = "无流控制"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
Magic Packet = "Magic Packet唤醒模式"
Pattern Match = "Pattern Match唤醒模式"
Mag Pack Patt Match = "Magic Packet 和Pattern Match唤醒模式"
Link Change = "Link Change唤醒模式"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; German (Standard)
[Strings.0407]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Netzwerkadresse"
HwCsum = "HW-Prüfsummenberechnung"
WakeUpCaps   = "Wake-up-Funktionen"
IntMod = "Interrupt-Moderation"
MaxIrq = "Max. IRQ pro Sek."
LogMsg = "Statusmeldungen protokollieren"
NumRcv = "Anzahl Empfangspuffer"
NumTx  = "Anzahl Sendepuffer"
RLMT  = "RLMT-Modus"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Bevorzugter Port"
On = "Ein"
Off = "Aus"
Non = "Keine"
Err = "Fehler"
Wrn = "Warnungen"
Sta = "Statusmeldungen"
All = "Alle Meldungen"
A = "A"
B = "B"
QoSSupA = "802.1p Unterstützung Port A"
QoSSupB = "802.1p Unterstützung Port B"
Slave = "Slave"
Master = "Master"
Auto = "Auto"
both = "Halb- und Vollduplex"
full = "Vollduplex"
half = "Halbduplex"
FlowCtrlA = "Datenflusskontrolle Port A"
FlowCtrlB = "Datenflusskontrolle Port B"
bothFC = "Asymmetrische und Symmetrische Datenflusskontrolle"
sym = "Symmetrische Datenflusskontrolle"
asym = "Asymmetrische Datenflusskontrolle"
noFc = "Keine Datenflusskontrolle"
Autosense = "Automatische Erkennung"
10MHD = "10 Mbit/s Halbduplex"
10MFD = "10 Mbit/s Vollduplex"
100MHD = "100 Mbit/s Halbduplex"
100MFD = "100 Mbit/s Vollduplex"
Magic Packet = "Magic Packet"
Pattern Match = "Pattern Match"
Mag Pack Patt Match = "Magic Packet und Pattern Match"
Link Change = "Link Change"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; undefined
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Dirección de red"
HwCsum = "Suma de comprobación del hardware"
WakeUpCaps   = "Capacidades de reactivación"
IntMod = "Moderación de interrupción"
MaxIrq = "IRQ máx. por seg."
LogMsg = "Mensajes de estado del registro"
NumRcv = "Número de búferes de recepción"
NumTx  = "Número de búferes de transmisión"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Puerto preferido"
On = "Encendido"
Off = "Apagado"
Non = "Ninguna"
Err = "Errores"
Wrn = "Advertencias"
Sta = "Mensajes de estado"
All = "Todos los mensajes"
A = "A"
B = "B"
QoSSupA = "Puerto A de soporte 802.1p"
QoSSupB = "Puerto B de soporte 802.1p"
Slave = "Secundario"
Master = "Maestro"
Auto = "Automático"
both = "Dúplex media y completa"
full = "Dúplex completa"
half = "Dúplex media"
FlowCtrlA = "Puerto A de control de flujo"
FlowCtrlB = "Puerto B de control de flujo"
bothFC = "Control de flujo simétrico y asimétrico"
sym = "Control de flujo simétrico"
asym = "Control de flujo simétrico"
noFc = "Sin control de flujo"
Autosense = "Orientación automática"
10MHD = "Dúplex media de 10Mbps"
10MFD = "Dúplex completa de 10Mbps"
100MHD = "Dúplex media de 100Mbps"
100MFD = "Dúplex completa de 100Mbps"
Magic Packet = "Paquete mágico"
Pattern Match = "Coincidencia de modelo"
Mag Pack Patt Match = "Paquete mágico y Coincidencia de modelo"
Link Change = "Cambio de enlace"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; undefined
[Strings.040C]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Adresse réseau"
HwCsum = "Contrôle de parité du matériel"
WakeUpCaps   = "Capacités de réveil"
IntMod = "Modération de l'interruption"
MaxIrq = "IRQ max. par seconde"
LogMsg = "Messages d'état du journal"
NumRcv = "Nombre de tampons de réception"
NumTx  = "Nombre de tampons de transmission"
RLMT  = "Mode RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Port préféré"
On = "Actif"
Off = "Inactif"
Non = "Aucun"
Err = "Erreurs"
Wrn = "Avertissements"
Sta = "Messages d'état"
All = "Tous les messages"
A = "A"
B = "B"
QoSSupA = "802.1p Support Port A"
QoSSupB = "802.1p Support Port B"
Slave = "Slave"
Master = "Master"
Auto = "Automatique"
both = "Semi-duplex et duplex intégral"
full = "Duplex intégral"
half = "Semi-duplex"
FlowCtrlA = "Contrôle de flux Port A"
FlowCtrlB = "Contrôle de flux Port B"
bothFC = "Contrôle de flux asymétrique et symétrique"
sym = "Contrôle de flux symétrique"
asym = "Contrôle de flux asymétrique"
noFc = "Pas de Contrôle de flux"
Autosense = "Détection automatique"
10MHD = "10 Mbits/s Semi-duplex"
10MFD = "10 Mbits/s Duplex intégral"
100MHD = "100 Mbits/s Semi-duplex"
100MFD = "100 Mbits/s Duplex intégral"
Magic Packet = "Magic Packet"
Pattern Match = "Pattern Match"
Mag Pack Patt Match = "Magic Packet et Pattern Match"
Link Change = "Link Change"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Italian (Standard)
[Strings.0410]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Indirizzo di rete"
HwCsum = "Checksumming hardware"
WakeUpCaps   = "Funzioni Wake Up "
IntMod = "Moderazione interrupt"
MaxIrq = "Max IRQ per sec"
LogMsg = "Messaggi di stato registro"
NumRcv = "Numero di buffer di ricezione"
NumTx  = "Numero di buffer di trasmissione"
RLMT  = "Modalità RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta preferita"
On = "On"
Off = "Off"
Non = "Nessuno"
Err = "Errori"
Wrn = "Avvertenze"
Sta = "Messaggi di stato"
All = "Tutti i messaggi"
A = "A"
B = "B"
QoSSupA = "802.1p Supporto Porta A"
QoSSupB = "802.1p Supporto Porta B"
Slave = "Slave"
Master = "Master"
Auto = "Auto"
both = "Half duplex e full duplex"
full = "Full duplex"
half = "Half duplex"
FlowCtrlA = "Controllo flusso Porta A"
FlowCtrlB = "Controllo flusso Porta B"
bothFC = "Controllo di flusso asimmetrico e simmetrico"
sym = "Controllo di flusso simmetrico"
asym = "Controllo di flusso asimmetrico"
noFc = "Nessun controllo di flusso"
Autosense = "Autoriconoscimento"
10MHD = "10Mbps half duplex"
10MFD = "10Mbps full duplex"
100MHD = "100Mbps half duplex"
100MFD = "100Mbps full duplex"
Magic Packet = "Magic Packet"
Pattern Match = "Criterio di ricerca"
Mag Pack Patt Match = "Magic Packet e criterio di ricerca"
Link Change = "Cambio collegamento"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Japanese
[Strings.0411]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "ネットワークアドレス"
HwCsum = "ハードウェアのチェック サム"
WakeUpCaps   = "ウェイク アップ機能"
IntMod = "割り込み節度"
MaxIrq = "毎秒最大 IRQ"
LogMsg = "ログ ステータス メッセージ"
NumRcv = "受信バッファ数"
NumTx  = "転送バッファ数"
RLMT  = "RLMTモード"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "優先ポート"
On = "オン"
Off = "オフ"
Non = "なし"
Err = "エラー"
Wrn = "警告"
Sta = "ステータス メッセージ"
All = "全てのメッセージ"
A = "A"
B = "B"
QoSSupA = "802.1p サポート ポート A"
QoSSupB = "802.1p サポート ポート B"
Slave = "スレーブ"
Master = "マスタ"
Auto = "自動"
both = "半二重と全二重"
full = "全二重"
half = "半二重"
FlowCtrlA = "フロー制御ポート A"
FlowCtrlB = "フロー制御ポート B"
bothFC = "非対称的および対称的フロー制御"
sym = "対称的フロー制御"
asym = "非対称的フロー制御"
noFc = "フロー制御なし"
Autosense = "自動感知"
10MHD = "10Mbps 半二重"
10MFD = "10Mbps 全二重"
100MHD = "100Mbps 半二重"
100MFD = "100Mbps 全二重"
Magic Packet = "マジック パケット"
Pattern Match = "パターン マッチ"
Mag Pack Patt Match = "マジック パケットとパターン マッチ"
Link Change = "リンクの変更"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Korean
[Strings.0412]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "네트워크 주소"
HwCsum = "하드웨어 검사합계"
WakeUpCaps   = "시스템 켜기 기능"
IntMod = "인터럽트 완화"
MaxIrq = "초당 최대 IRQ"
LogMsg = "로그 상태 메시지"
NumRcv = "수신 버퍼 수"
NumTx  = "송신 버퍼 수"
RLMT  = "RLMT 모드"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "기본 설정 포트"
On = "켜기"
Off = "끄기"
Non = "없음"
Err = "오류"
Wrn = "경고"
Sta = "상태 메시지"
All = "모든 메시지"
A = "A"
B = "B"
QoSSupA = "802.1p 지원 포트 A"
QoSSupB = "802.1p 지원 포트 B"
Slave = "슬레이브"
Master = "마스터"
Auto = "자동"
both = "반이중 및 전이중"
full = "전이중"
half = "반이중"
FlowCtrlA = "흐름 제어 포트 A"
FlowCtrlB = "흐름 제어 포트 B"
bothFC = "비대칭 및 대칭 흐름 제어"
sym = "대칭 흐름 제어"
asym = "비대칭 흐름 제어"
noFc = "흐름 제어 없음"
Autosense = "자동 감지"
10MHD = "10Mbps 반이중"
10MFD = "10Mbps 전이중"
100MHD = "100Mbps 반이중"
100MFD = "100Mbps 전이중"
Magic Packet = "매직 패킷"
Pattern Match = "패턴 일치"
Mag Pack Patt Match = "매직 패킷 및 패턴 일치"
Link Change = "링크 변경"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Polish
[Strings.0415]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Adres sieciowy"
HwCsum = "Podsumowanie sprawdzenia sprzętu"
WakeUpCaps   = "Funkcje budzenia"
IntMod = "Moderacja przerwania"
MaxIrq = "Maks. IRQ na sek."
LogMsg = "Zapisywanie komunikatów o statusie"
NumRcv = "Liczba buforów odbiorczych"
NumTx  = "Liczba buforów nadawczych"
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferowany port"
On = "Włączone"
Off = "Wyłączone"
Non = "Żadne"
Err = "Błędy"
Wrn = "Ostrzeżenia"
Sta = "Komunikaty o stanie"
All = "Wszystkie komunikaty"
A = "A"
B = "B"
QoSSupA = "802.1p Obsługa Port A"
QoSSupB = "802.1p Obsługa Port B"
Slave = "Podrzędny"
Master = "Nadrzędny"
Auto = "Automatyczny"
both = "Pół- i pełny dupleks"
full = "Pełny dupleks"
half = "Pół- dupleks"
FlowCtrlA = "Kontrola przepływu danych Port A"
FlowCtrlB = "Kontrola przepływu danych Port B"
bothFC = "Asymetryczna i symetryczna kontrola przepływu danych"
sym = "Symetryczna kontrola przepływu danych"
asym = "Asymetryczna kontrola przepływu danych"
noFc = "Brak kontroli przepływu danych"
Autosense = "Automatyczne wykrywanie"
10MHD = "10 Mbps Półdupleks"
10MFD = "10 Mbps Pełen dupleks"
100MHD = "100 Mbps Półdupleks"
100MFD = "100 Mbps Pełen dupleks"
Magic Packet = "Magic Packet"
Pattern Match = "Pattern Match"
Mag Pack Patt Match = "Magic Packet i Pattern Match"
Link Change = "Zmiana łącza"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Portuguese (Brazil)
[Strings.0416]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Endereço de Rede"
HwCsum = "Teste Lógico de Hardware"
WakeUpCaps   = "Capacidades de Despertar"
IntMod = "Moderação de Interrupção"
MaxIrq = "IRQ Máx por Seg"
LogMsg = "Registrar Mensagens de Estado"
NumRcv = "Número de Buffers de Recepção"
NumTx  = "Número de Buffers de Transmissão"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta Preferida"
On = "Ligado"
Off = "Desligado"
Non = "Nenhum"
Err = "Erros"
Wrn = "Avisos"
Sta = "Mensagens de Estado"
All = "Todas as Mensagens"
A = "A"
B = "B"
QoSSupA = "Porta A Suporte 802.1p"
QoSSupB = "Porta B Suporte 802.1p"
Slave = "Escravo"
Master = "Mestre"
Auto = "Auto"
both = "Dúplex semi e completo"
full = "Dúplex Completo"
half = "Semi Dúplex"
FlowCtrlA = "Controle de Fluxo Porta A"
FlowCtrlB = "Controle de Fluxo Porta B"
bothFC = "Controle de Fluxo Simétrico e Assimétrico"
sym = "Controle de Fluxo Simétrico"
asym = "Controle de Fluxo Assimétrico"
noFc = "Sem Controle de Fluxo"
Autosense = "Autodetecção"
10MHD = "Semi Dúplex 10Mbps"
10MFD = "Dúplex Completo 10Mbps"
100MHD = "Semi Dúplex 100Mbps"
100MFD = "Dúplex Completo100Mbps"
Magic Packet = "Pacote Mágico"
Pattern Match = "Padrão Igualado"
Mag Pack Patt Match = "Pacote Mágico e Padrão Igualado"
Link Change = "Troca de Vínculo"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"


; Russian
[Strings.0419]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
Marvell = "Marvell"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------

NetAddress   = "Сетевой адрес"
HwCsum = "Аппаратный контроль суммы"
WakeUpCaps   = "Возможности пробуждения"
IntMod = "Управление прерываниями"
MaxIrq = "Макс. IRQ - шт/сек."
LogMsg = "Записывать статусные сообщения"
NumRcv = "Число буферов приема"
NumTx  = "Число буферов передачи"
RLMT  = "Режим RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Предпочтительный порт"
On = "Вкл."
Off = "Выкл."
Non = "Нет"
Err = "Ошибки"
Wrn = "Предупреждения"
Sta = "Статусные сообщения"
All = "Все сообщения"
A = "A"
B = "B"
QoSSupA = "Поддержка 802.1p, порт A"
QoSSupB = "Поддержка 802.1p, порт B"
Slave = "Ведомый"
Master = "Ведущий"
Auto = "Авто"
both = "Полудуплекс и полный дуплекс"
full = "Полный дуплекс"
half = "Полудуплекс"
FlowCtrlA = "Управление потоком данных, порт A"
FlowCtrlB = "Управление потоком данных, порт B"
bothFC = "Асимметричное и симметричное управление потоком данных"
sym = "Симметричное управление потоком данных"
asym = "Асимметричное управление потоком данных"
noFc = "Без управления потоком данных"
Autosense = "Автоопределение"
10MHD = "10 Мбит/с, полудуплекс"
10MFD = "10 Мбит/с, полный дуплекс"
100MHD = "100 Мбит/с, полудуплекс"
100MFD = "100 Мбит/с, полный дуплекс"
Magic Packet = "Magic Packet"
Pattern Match = "Соответствие шаблону"
Mag Pack Patt Match = "Magic Packet и соответствие шаблону"
Link Change = "Смена канала"
BatSpeed = "BatterySpeedSettings"
Fast = "SmartSpeedDown"
Gig = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
WakeFromShut = "Wake From Shutdown"
Enabled = "Enabled"
Disabled = "Disabled"
FlowCtrl = "FlowControl"
TcpSegmentation = "TCP Segmentation"
SpeedDuplex = "Speed & Duplex"
SpeedDuplexA = "Speed & Duplex Port A"
SpeedDuplexB = "Speed & Duplex Port B"
QoSSup = "802.1p Support"
MaxFrSize    = "Jumbo Frames"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"


Yukon.DeviceDesc4320 = "Marvell Yukon 88E8001/8003/8010 PCI Gigabit Ethernet Controller"
Yukon.DeviceDesc4340 = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4341 = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4342 = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4343 = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344SX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345SX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346SX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347SX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4344LX = "Marvell Yukon 88E8021 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4345LX = "Marvell Yukon 88E8022 PCI-X ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4346LX = "Marvell Yukon 88E8061 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4347LX = "Marvell Yukon 88E8062 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4350 = "Marvell Yukon 88E8035 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4351 = "Marvell Yukon 88E8036 PCI-E Fast Ethernet Controller"
Yukon.DeviceDesc4360 = "Marvell Yukon 88E8052 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4361 = "Marvell Yukon 88E8050 PCI-E ASF Gigabit Ethernet Controller"
Yukon.DeviceDesc4362 = "Marvell Yukon 88E8053 PCI-E Gigabit Ethernet Controller"
Yukon.DeviceDescGen = "Generic Marvell Yukon Chipset based Gigabit Ethernet Controller"

SK-9872.DeviceDesc = "SysKonnect SK-9872 Gigabit Ethernet Server Adapter (SK-NET GE-ZX dual link)"
SK-9871-V2.DeviceDesc = "SysKonnect SK-9871 V2.0 Gigabit Ethernet 1000Base-ZX Adapter, PCI64, Fiber ZX/SC"
SK-9871.DeviceDesc = "SysKonnect SK-9871 Gigabit Ethernet Server Adapter (SK-NET GE-ZX)"
SK-9862.DeviceDesc = "SysKonnect SK-9862 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition dual link)"
SK-9861-V2.DeviceDesc = "SysKonnect SK-9861 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/VF-45"
SK-9861.DeviceDesc = "SysKonnect SK-9861 Gigabit Ethernet Server Adapter (SK-NET GE-SX Volition)"
SK-9851-V2.DeviceDesc = "SysKonnect SK-9851 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/MTRJ"
SK-9844.DeviceDesc = "SysKonnect SK-9844 Gigabit Ethernet Server Adapter (SK-NET GE-SX dual link)"
SK-9843-V2.DeviceDesc = "SysKonnect SK-9843 V2.0 Gigabit Ethernet 1000Base-SX Adapter, PCI64, Fiber SX/SC"
SK-9843.DeviceDesc = "SysKonnect SK-9843 Gigabit Ethernet Server Adapter (SK-NET GE-SX)"
SK-9842.DeviceDesc = "SysKonnect SK-9842 Gigabit Ethernet Server Adapter (SK-NET GE-LX dual link)"
SK-9841-V2.DeviceDesc = "SysKonnect SK-9841 V2.0 Gigabit Ethernet 1000Base-LX Adapter, PCI64, Fiber LX/SC"
SK-9841.DeviceDesc = "SysKonnect SK-9841 Gigabit Ethernet Server Adapter (SK-NET GE-LX)"
SK-9822.DeviceDesc = "SysKonnect SK-9822 Gigabit Ethernet Server Adapter (SK-NET GE-T dual link)"
SK-9821-V2.DeviceDesc = "SysKonnect SK-9821 V2.0 Gigabit Ethernet 10/100/1000Base-T Adapter, PCI64, Copper RJ-45"
SK-9821.DeviceDesc = "SysKonnect SK-9821 Gigabit Ethernet Server Adapter (SK-NET GE-T)"
SK-9521.DeviceDesc = "SysKonnect SK-9521 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9521-V2.DeviceDesc = "SysKonnect SK-9521 V2.0 10/100/1000Base-T Adapter, PCI 32bit, Copper RJ-45"
RDK-8012.DeviceDesc = "SysKonnect Marvell RDK-8012 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8011.DeviceDesc = "SysKonnect Marvell RDK-8011 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8009.DeviceDesc = "SysKonnect Marvell RDK-8009 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8008.DeviceDesc = "SysKonnect Marvell RDK-8008 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8007.DeviceDesc = "SysKonnect Marvell RDK-8007 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8006.DeviceDesc = "SysKonnect Marvell RDK-8006 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8004.DeviceDesc = "SysKonnect Marvell RDK-8004 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8003.DeviceDesc = "SysKonnect Marvell RDK-8003 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8002.DeviceDesc = "SysKonnect Marvell RDK-8002 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
RDK-8001.DeviceDesc = "SysKonnect Marvell RDK-8001 10/100/1000Base-T Adapter, PCI, Copper RJ-45"
SK-9E21.DeviceDesc = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter, Copper RJ-45"

SKYukon.DeviceDesc9E21D = "SysKonnect SK-9E21D 10/100/1000Base-T Adapter,PCI-Express" 
SKYukon.DeviceDesc9E21 = "SysKonnect SK-9E21 10/100/1000Base-T Server Adapter, PCI-Express" 
SKYukon.DeviceDesc9E22 = "SysKonnect SK-9E22 10/100/1000Base-T Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E81 = "SysKonnect SK-9E81 1000Base-SX Server Adapter,PCI-Express"
SKYukon.DeviceDesc9E82 = "SysKonnect SK-9E82 1000Base-SX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9E91 = "SysKonnect SK-9E91 1000Base-LX Server Adapter,PCI-Express" 
SKYukon.DeviceDesc9E92 = "SysKonnect SK-9E92 1000Base-LX Dual Port Server Adapter, PCI-Express"
SKYukon.DeviceDesc9S21 = "SysKonnect SK-9S21 10/100/1000Base-T Server Adapter, PCI-X, Copper RJ-45" 
SKYukon.DeviceDesc9S22 = "SysKonnect SK-9S22 10/100/1000Base-T Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S81 = "SysKonnect SK-9S81 1000Base-SX Server Adapter,PCI-X" 
SKYukon.DeviceDesc9S82 = "SysKonnect SK-9S82 1000Base-SX Dual Port Server Adapter, PCI-X"
SKYukon.DeviceDesc9S91 = "SysKonnect SK-9S91 1000Base-LX Server Adapter,PCI-X"
SKYukon.DeviceDesc9S92 = "SysKonnect SK-9S92 1000Base-LX Dual Port Server Adapter, PCI-X" 
yk51x86.DriverDesc	= "NDIS5.1 Miniport Driver for Marvell Yukon Ethernet Controller"

