; Windows USB CDC ACM Setup File

; Based on INF template which was:
;     Copyright (c) 2000 Microsoft Corporation
;     Copyright (c) 2007 Microchip Technology Inc.
; likely to be covered by the MLPL as found at:
;    <http://msdn.microsoft.com/en-us/cc300389.aspx#MLPL>.
; For use only on Windows operating systems.
; Customized for Telit products. 15/12/2017

[Version]
Signature     = "$Windows NT$"
Class         = Ports
ClassGuid     = {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider      = %provider_name%
DriverVer     = 11/05/2013,5.1.2600.0
CatalogFile   = telit_cdc_acm.cat
PnpLockdown   = 1

[Manufacturer]
%provider_name%    =DeviceList, NTx86, NTamd64


;------------------------------------------------------------------------------
;  32bit Sections
;------------------------------------------------------------------------------

[DriverInstall.nt]
include=mdmcpq.inf
AddReg=DriverInstall.nt.AddReg
; No sys copyfiles - the sys files are already in-build 
; (part of the operating system).

[DriverInstall.nt.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBSER.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.nt.Services]
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\USBSER.sys

;------------------------------------------------------------------------------
;  64bit Sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64]
include=mdmcpq.inf
AddReg=DriverInstall.NTamd64.AddReg
; No sys copyfiles - the sys files are already in-build 
; (part of the operating system).

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBSER.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\USBSER.sys

;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------

[SourceDisksFiles]
[SourceDisksNames]

[DeviceList.NTx86]
%USB_PORT0%=DriverInstall, USB\VID_1bc7&PID_2300&MI_02
%USB_PORT1%=DriverInstall, USB\VID_1bc7&PID_2300&MI_04
%USB_PORT2%=DriverInstall, USB\VID_1bc7&PID_2300&MI_06
%DESCRIPTION%=DriverInstall, USB\VID_216f&PID_0051

[DeviceList.NTamd64]
%USB_PORT0%=DriverInstall, USB\VID_1bc7&PID_2300&MI_02
%USB_PORT1%=DriverInstall, USB\VID_1bc7&PID_2300&MI_04
%USB_PORT2%=DriverInstall, USB\VID_1bc7&PID_2300&MI_06
%DESCRIPTION%=DriverInstall, USB\VID_216f&PID_0051

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings]
provider_name       = "Telit"
USB_PORT0           = "USB0"
USB_PORT1           = "USB1"
USB_PORT2           = "USB3"
DESCRIPTION         = "CDC-ACM"
SERVICE             = "USB RS-232 Emulation Driver"
SourceDisk          = "USBSER Gadget Driver Install Disk"
